# Ladies Large Print Watch ES0044

# Product Instructions

# General Description

This ladies large print watch has a silver rim with a clear white face, bold black numbers and black hands. It is fitted with a white crocodile effect strap.  
It is 5 ATM water resistant meaning that it is splash and rain resistant, it will resist moisture and can also be worn while swimming in shallow water or showering.

# Instructions

# Product features

**5 ATM/50 meters water resistant** - You can wear this watch in the shower or surface swimming; please ensure that the crown is tightly pushed into the watch.

Please note: This watch is not suitable for diving, or situations of high steam capacity. This includes very hot showers, saunas or hot tubs.

## Orientation

Position the watch in front of you so that the straps are vertically aligned, pointing up and down. On the outer edge of the watch case, on the right hand side you will find a round, metal winder that protrudes out from the rest of the watch. This is the crown that is used to set the time.

**Setting the time**

Locate the crown on the outer edge of the watch casing, on the right hand side. Pull the crown out from the watch until you hear a small click, rotate the crown to set the time, and then push in towards the casing to activate. The watch is now set.

# Hints and Tips

## Batteries

* This watch uses one 377 battery.
* It is strongly recommended that a qualified person, such as a trained jeweller or watch specialist should fit new batteries to avoid any damage to the watch.
* To replace the battery a qualified person should remove the back. Then remove the old battery and insert 1 x 377 new battery. Observe polarity (+/-) sign when installing batteries.
* Use only designated battery type. Do not use re-chargeable batteries.
* Read instructions carefully and install batteries correctly observing the polarity (+/-) sign to avoid leakage.
* Do not attempt to recharge non-rechargeable batteries.
* Remove batteries from the product when it will not be used for an extended period of time to avoid leakage.
* Remove exhausted battery to avoid leakage.
* Do not short out battery contacts.
* Do not dispose of batteries in fire.
* Do not immerse electrically operated products in water or other liquid. Wipe clean only.