Tactile Watch with Diamante Bezel ES0047

Product Instructions

# General Description

This elegant, stainless steel ladies watch has a charcoal toned dial which is complimented by clear crystals, to decorate the bezel.

It has a tactile mark indicating 12 o'clock, two dots to indicate 3, 6 and 9 o'clock and one dot to indicate each hour in-between; completed with the lid opening at the 6 o'clock position.

# Instructions

## Special warning

Each watch is fitted with a "sleeper", which is a small piece of plastic fitted in between the watch and the winder, and prevents the watch from working, and subsequently the battery from draining while in storage.

Once the "sleeper" has been removed, turn the winder to set the time and then push it back in and the watch will now be activated.

**Do NOT set the time by rotating the hands as this will break the hands. Use the winder only.**

## Orientation

The watches have a round-shaped face. The lid opens at the 6 o’clock position and the winder is on the right at the 3 o’clock position.

The tactile marks on the face are as follows:

12 o’clock – long thin bar

3, 6 and 9 o’clock – two dots

Every other position – single dot

This watch has a metallic bracelet straps have two wires attached to the strap and plastic holder within the packaging, to prevent them from moving and possibly getting damaged in transit. These will need to be removed before use.

The clasp on the metallic bracelet strap is located centrally, either side of the bracelet links. To undo the clasp, unclip the small catch over the clasp and pull it up. You can feel where the front of the catch is as there is a small recessed area, semi-circular in shape, in front of it. Once lifted feel underneath the opened catch and you will feel a small metallic catch protruding. This is about 1cm away from the semi-circular recess. Pull this catch away from the other opened catch and the strap will open. Simply slide the watch with opened strap over your wrist and then fold the opened part of the strap until it clicks shut. Finally, close the catch back over the clasp.

The bracelet is adjustable. We recommend that links are removed or added by a jeweller or watch specialist as it requires tools to remove and replace the spring loaded adjustment bar. The spring loaded adjustment bar can be moved into different location holes to adjust the size of the bracelet to fit most wrists.

## Battery replacement

It is recommended that only watch specialists or jewellers change the battery. These watches are all fitted with a silver oxide SR626SW (SR66/377) battery.