# Braille keyboard stickers ES0134

# Product Instructions

# General description

A comprehensive set of 72 adhesive-backed overlays with raised Braille markings for a standard computer keyboard. Made from durable materials the set includes all letter and number keys, as well as most of the common function keys.

# Items supplied

* Braille keyboard stickers
* Wooden application tool
* Instructions

# Specification

Set of 72 braille self-adhesive overlays

Includes keys: all letter and number keys, F1 through F10, Escape, Home, Insert, Control, Alt, Delete, Enter, Up/ Down arrows and End

Includes wooden tool to aid application

Each sticker is W11mm x H18mm

Sighted assistance may be required to apply.

Leaving the original letters on the keyboard readable, all the family can use the keyboard with these overlays.

# Orientation

Position the sheet in front of you so that the Braille can be felt on the surface. Rotate so that “a” can be felt in the top left corner.

# Getting started

It is recommended not to use fingers to apply these stickers as this may remove the self-adhesive. It is recommended to use tweezers.

# Applying the stickers

With your computer turned off, clean the tops of the keys with an alcohol pad or wipe (not supplied). If using tweezers lift the sticker label from the backing sheet, touching as little of the adhesive on the back as possible. Lightly place the label over the correct, corresponding key, ensuring the label is central. If using your fingers to remove and place the labels (not recommended), handle the labels by their edges.

**Please note:** If the product is put onto the wrong key and is re-applied to a different one, the adhesive will not be as effective.

After each label is positioned, rub it down firmly with the provided wooden application tool ensuring that you firm particularly around the edges.